**SaddleRoller Series Pipe Supports**

Engineering Specification & Detail:

Support for pipe, conduit, refrigeration lines shall be MAPA Products SaddleRoller Supports. Pipe support base shall combine UV protected 33% fiberglass reinforced 6/6 Nylon and Height Extender which securely attaches to the base to achieve a maximum height of 4” and is designed to allow for a “free-standing”, “non-penetration” installation that may incorporate readily available accessories. Provide support with adhered pad installed in accordance with the project manager or other designated roofing professional.

